Lernout & Hauspie Speech Products NV
Flanders Language Valley 50
B-8900 Ieper, Belgium
Phone: +32 57 22 8888  Fax: +32 57 20 8489

Product Release Package
Product Name:	L&H PCMM TTS3000 SDK for Windows Desktop Platform Jpn.JPN SAPI5 1.00 
	Final
Version:	1.00
Date:	20 November 2000
Contract ref.:	97126/U

Contents
•	Product Release Note

Lernout & Hauspie Speech Products NV
Flanders Language Valley 50
B-8900 Ieper, Belgium
Phone: +32 57 22 8888  Fax: +32 57 20 8489

Release Note
Product Name:		L&H PCMM TTS3000 SDK for Windows Desktop Platform Jpn.JPN SAPI5 1.00 
Final
Product Number:	A96502
Version:	1.00 
Date:	20 November 2000
Contract ref.:	97126/U

This note provides a list of all items, software and documentation included, L&H product and version numbers and installation guidelines.

This release contains the PC implementation of the L&H TTS3000 JPJ (Japanese) for Windows Desktop . The L&H TTS3000 JPJ for Windows Desktop of the Text-to-Speech system is delivered as a set of DLL’s.  Further specifications are given below.

Deliverables
Merge Module:
•	LHTTS3000SHAERED.MSM : Merge module for common components 
•	LHTTINT.MSM : Merge module for Japanese 

Items in LHTTS3000SHARED.MSM:
•	TTSCORE.DLL : Core Module for L&H TTS3000
•	TTS3000.HDR : Information file for TTS3000
•	LHCOM01A.DLL : Common resource module

Items in LHTTINT.MSM:
•	JPJT3S51.DLL : Japanese SAPI5 Interface module
•	JPJTSTPP.DLL : Normal text preprocessing module
•	JPJTSTPP.HDR : Information file for JPJTSTPP.DLL
•	JPJTG2P.DLL : Linguistic processing module 
•	JPJTG2P.HDR : Information file for JPJTG2P.DLL 
•	JPJT11F1.DLL : Naoko voice module
•	JPJT11F1.HDR : Information file for JPJT11F1.DLL 
•	NAOKO.DAT : Data file for JPJT11F1.DLL 
•	JPJT11M1.DLL : Kenji voice module
•	JPJT11M1.HDR : Information file for JPJT11M1.DLL 
•	KENJI.DAT : Data file for JPJT11M1.DLL 

System requirements
•	Intel Pentium based PC (90MHz) or higher
•	8 Mb RAM (16 Mb RAM is recommended for Windows NT). TTS system requires about 2M bytes
•	CD-ROM drive
•	6 Mb hard disk space to install and run the selected products. SoundBlaster 16 compatible audio device
•	MS Windows 95/98 or MS Windows NT 4.0 or Windows2000

Installation procedure
Use delivered merge module

Changes
•	Language-independent:
•	This version consists of two merges, LHTTS3000SHARED.MSM and LHTTINT.MSM. LHTTS3000SHARED.MSM merge module contains language independent components.
•	Context XML tags are supported in this version.

•	Language-dependent:
None

Limitations and Features not implemented
This version does not support all XML tags. The following tags are not supported:
•	EMPH

 2000 L&H™. All rights reserved.