********************************************************************************************

HISTORY FILE FOR EP2BRES and related GPD's - Most recent at the top

********************************************************************************************
Still TODO

EPLQ680/680P:
- Support back rear manual insertion
- 0 margins on Fanfold papers (SEC specs)

EP2BRES.DLL:
- Make xxxxxxPS fonts in NLSP mode (need font width information)
- Add new CP's (wait for MDT update for CP support)

********************************************************************************************
Modified on December 15 by MarcM
All new GPD's (2080/2180/570e/580e/680/680Pro) version numbers 1.0 (Initial Release)
All updated GPD's (2070/2170/670) version numbers 1.1 (Update since W2K package)

EPLQ2070.GPD:
- Based on EPLQ2080.GPD, changed names and PrintRate

EPLQ2170.GPD:
- Based on EPLQ2180.GPD, changed names and PrintRate

EPLQ670.GPD:
- Based on EPLQ680.GPD, changed names, PrintRate and removed extended ESC EM commands

EPLQ2080.GPD:
- Changed all top/bottom margins on Fanfold papers to 4.2/4.2 (60/60)
- Fixed CUSTOMSIZE MaxPrintable area and margins to 4.2/4.2 (60/60)
- Corrected PrintableArea for A3_Rotated and changed srting ID 256 to 254
- Added TC_UA_ABLE in TextCaps
- Added Font 56 (SDRAFTPS) in Standard mode and Font 97 in NLSP (SDRAF10N)
- Changed EPSON into Epson

EPLQ2180.GPD:
- Changed all top/bottom margins on Fanfold papers to 4.2/4.2 (60/60)
- Fixed CUSTOMSIZE MaxPrintable area and margins to 4.2/4.2 (60/60)
- Corrected PrintableArea for A3_Rotated and changed srting ID 256 to 254
- Added TC_UA_ABLE in TextCaps
- Added Font 56 (SDRAFTPS) in Standard mode and Font 97 in NLSP (SDRAF10N)
- Changed EPSON into Epson

EPLQ570E.GPD:
- Changed all top/bottom margins on Fanfold papers to 4.2/4.2 (60/60)
- Fixed CUSTOMSIZE margins to 4.2/4.2 (60/60)
- Added TC_UA_ABLE in TextCaps
- Added Font 56 (SDRAFTPS) in Standard mode and Font 97 in NLSP (SDRAF10N)
- Changed EPSON into Epson

EPLQ580.GPD:
- Changed all top/bottom margins on Fanfold papers to 4.2/4.2 (60/60)
- Fixed CUSTOMSIZE margins to 4.2/4.2 (60/60)
- Added TC_UA_ABLE in TextCaps
- Added Font 56 (SDRAFTPS) in Standard mode and Font 97 in NLSP (SDRAF10N)
- Changed EPSON into Epson

EPLQ680P.GPD:
- Added TC_UA_ABLE in TextCaps
- Added Font 56 (SDRAFTPS) in Standard mode and Font 97 in NLSP (SDRAF10N)
- Changed EPSON into Epson

EPLQ680.GPD:
- Added TC_UA_ABLE in TextCaps
- Added Font 56 (SDRAFTPS) in Standard mode and Font 97 in NLSP (SDRAF10N)
- Changed EPSON into Epson

EP2BRES.DLL:
- Copied SDRAFT10.UFM to SDRAF10N.UFM (ID 97) and changed default CTT to 2
- Added LQ-670, LQ-2070 and LQ-2170 into MDW

********************************************************************************************
Modified on December 14 by MarcM
All GPD's version numbers 1.0 (Initial Release)

EPLQ2080.GPD:
- Based on EPLQ2180.GPD, changed names and PrintRate

EPLQ2180.GPD:
- Based on ESCP58.GPD
- Removed all *switch: InputBin from and co-mments from PaperSize 
- Renamed all PaperSize.OptionX to readable english (standard among all GPD's)
- Added FontSupport feature (Standard, NLSP or NoFont) and switch DeviceFonts, DefaultFont and DefaultCTT accordingly
- Added all Printer Font support and commands (same as EPLQ580)
- Added PrintQuality feature (same as EPLQ580)
- Renumbered rcNameID for all PaperSize to match EP2BRES.RC
- Added ESC (t command in CmdStartDoc to load PC437 as table 1 and select it.
- Added PrintRate, PrintRateUnit and copyright information

EPLQ570E.GPD:
- Based on EPLQ580.GPD, changed names and removed NLSP support

EPLQ580.GPD:
- Renamed all PaperSize.OptionX to readable english (standard among all GPD's)
- Added FontSupport feature (Standard, NLSP or NoFont) and switch DeviceFonts, DefaultFont and DefaultCTT accordingly
- Added CmdUnderlineOn and CmdUnderlineOff
- Added PrintRate, PrintRateUnit and copyright information

EPLQ680P.GPD:
- Based on EPLQ680.GPD and changed names

EPLQ680.GPD:
- Renamed all PaperSize.OptionX to readable english (standard among all GPD's)
- Added FontSupport feature (Standard, NLSP or NoFont) and switch DeviceFonts, DefaultFont and DefaultCTT accordingly
- Added ESC (t command in CmdStartDoc to load PC437 as table 1 and select it.
- Added PrintRate, PrintRateUnit and copyright information

EP2BRES.DLL:
- Copied all COURxx.UFM to COURxxN.UFM (ID 57~63) and changed default CTT to 2
- Copied all DRAFTxx.UFM to DRAFTxxN.UFM (ID 64~70) and changed default CTT to 2
- Copied all PRESTxx.UFM to PRESTxxN.UFM (ID 71~76) and changed default CTT to 2
- Copied all ROMANxx.UFM to ROMANxxN.UFM (ID 77~83) and changed default CTT to 2
- Copied all SANSxx.UFM to SANSxxN.UFM (ID 84~90) and changed default CTT to 2
- Copied all SCRIPTxx.UFM to SCRIPNxx.UFM (ID 91~96) and changed default CTT to 2
- Changed EPNLSP39.GTT to ID 2, EPSTD13.GTT to ID 1 and deleted EPSONEUR.GTT
- Added CopePage 1252 and defined only UC+20AC (Euro) in PC858 (d5H) for both EPNLSP39.GTT and EPSTD13.GTT
- Added strings 255~257 (from LQ-2x80) and 272~274 (FontSupport feature)
- Added LQ-2080, LQ-570e and LQ-680Pro into MDW

********************************************************************************************
Modified on December 13 by MarcM
All GPD's version numbers 1.0 (Initial Release)

EPLQ580.GPD:
- Added ESC (t command in CmdStartDoc to load PC437 as table 1 and select it.

EPLQ680.GPD:
- No change.

EP2BRES.DLL:
- Moved MDW to version 7 (thanks new MDT 001207) and cannot revert back to version 6
- Added EPSTD13.GTT (PC850+437) and EPNLSP39.GTT (PC850+437+869+857+866+864)
- Changed EPNLSP39.GTT to ID 1 for testing

********************************************************************************************
Modified on December 12 by MarcM
All GPD's version numbers 1.0 (Initial Release)

EPLQ580.GPD:
- Based on ESCP5B.GPD
- Renumbered PaperSize.Option8~10 to 10~12
- Renumbered PaperSize.Option13~17 to 16~20
- Removed all *switch: InputBin from and co-mments from PaperSize 
- Renumbered rcNameID 266~270 to 267~271
- Renumbered fonts 56 to 55

EPLQ680.GPD:
- Based on ESCP5EH.GPD
- Renumbered rcNameID 262~266 to 261~265 and 261 to 266

EP2BRES.DLL:
- Based on ESCP5E.DLL + all UFM/GTT from ESCP5E
- Removed strings 1~2
- Renumbered strings 262~266 to 261~265 and 261 to 266
- Removed GTT 2~4
- Added UFM 56 DRAFTPS.UFM