********************************************************************************************

HISTORY FILE FOR EP2BRES and related GPD's - Most recent at the top

********************************************************************************************
Still TODO

EP2BRES.DLL:
- Make xxxxxxPS fonts in NLSP mode (need font width information)
- Add new CP's (wait for MDT update for CP support)
- Move FX-2170/2180/880/1180 to new driver

********************************************************************************************
Modified on December 15 by MarcM
All new GPD's version numbers 1.0 (Initial Release)

EPLX300P.GPD:
- Based on ESCP5D.GPD
- Removed all *switch: InputBin from and comments from PaperSize 
- Renamed all PaperSize.OptionX to readable english (standard among all GPD's)
- Added FontSupport feature (Standard, NLSP or NoFont) and switch DeviceFonts, DefaultFont and DefaultCTT accordingly
- Added PrintQuality feature
- Renumbered all strings to match EP9BRES.RC
- Added ESC (t command in CmdStartDoc to load PC437 as table 1 and select it.
- Added PrintRate, PrintRateUnit and copyright information

EPFX980.GPD:
- Based on ESCP5A.GPD
- Removed all *switch: InputBin from and comments from PaperSize 
- Renamed all PaperSize.OptionX to readable english (standard among all GPD's)
- Added FontSupport feature (Standard, NLSP or NoFont) and switch DeviceFonts, DefaultFont and DefaultCTT accordingly
- Added PrintQuality feature
- Renumbered all strings to match EP9BRES.RC
- Added ESC (t command in CmdStartDoc to load PC437 as table 1 and select it.
- Added PrintRate, PrintRateUnit and copyright information

EP9BRES.DLL:
- Based on ESCP5A.DLL
- Moved MDW to version 7 (thanks new MDT 001207) and cannot revert back to version 6
- Renumbered all strings same as EP2BRES
- Removed GTT 1~4
- Added EPSTD13.GTT (PC850+437) and EPNLSP39.GTT (PC850+437+869+857+866+864)
- Added CopePage 1252 and defined only UC+20AC (Euro) in PC858 (d5H) for both EPNLSP39.GTT and EPSTD13.GTT
- Copied all DRAFTxx.UFM to DRAFTxxN.UFM (ID 30~36) and changed default CTT to 2
- Copied all ROMANxx.UFM to ROMANxxN.UFM (ID 38~44) and changed default CTT to 2
- Copied all SANSxx.UFM to SANSxxN.UFM (ID 46~52) and changed default CTT to 2
- Copied all SDRAFTxx.UFM to SDRAFTxx.UFM (ID 54~58) and changed default CTT to 2
- Changed EPNLSP39.GTT to ID 2, EPSTD13.GTT to ID 1 and deleted EPSONEUR.GTT